Parallel opening fitting, manual

**concealed stays, for aluminium window systems**

1 manual parallel opening fitting,  
concealed stays, open inwards or outwards,  
for aluminium window system with a Euro groove

**Leaf dimensions**

max. flap height: 150 kg

max. flap height: 1,350 mm

max. flap height: 3,000 mm

max. opening width: 200 mm  
necessary rebate size: 17 x 23 mm

* Suitable for installation in the series profiles of various profile systems.
* Operation by means of 2 handle gears, one each on the left and right on the inside of the leaf - with a lift limiter.
* We recommend the use of a continuous push bar for leaves over 1,000 in width.
* Infinitely variable opening.
* Tandem-PX and PY stays concealed in the window rebate.
* Compact control stay used horizontally, concealed in the bottom rebate.
* Corrosion resistance according to **DIN EN 1670, Class 5**

**Optional design**

* The open leaf can be fixed by turning the handles.
* Additional horizontal interlock.

**Other elements needed**

* Handle gear for PAF fitting

**e.g. WSS parallel opening fitting, manual**