Top-hung fitting, manual

**concealed stay, for aluminium window systems with sash overlap**

1 manual top-hung fitting,  
concealed stays,  
for aluminium window system with a Euro groove and sash overlap.

**Leaf dimensions**

max. leaf weight: 136 kg

max. leaf width: 1,250 mm

max. leaf height: 2,200 mm

max. opening angle: 40°  
necessary rebate size: 17 mm (pay attention to the fall protection/man. operability)

* Suitable for installation in the series profiles of various profile systems.
* Operated by a handle drive at the bottom.
* With a push rod and corner linkage for vertical and horizontal locking pins at the top and sides - with lift limiter.
* Additional central interlocks are used in the upper horizontal area.
* Opening is to the right and left sides with 4-point stays.
* The size of the stays must match the leaf height and weight.
* With brake installed on the frame side.
* The height adjustment +/- 4 mm allows the fine adjustment of the leaf and gap size on the building site.
* All elements of fully corrosion-resistant materials.

**e.g. WSS top-hung fitting, manual**

**Optional design**

* The open leaf can be fixed by turning the handles.
* Additional horizontal interlock.

**Other elements needed**

* Window handle [Enter text]

***DANGER!****The max. leaf size is determined by the max. leaf weight of 136 kg.*