Fanlight tilt fitting AK 210/300, manual

**visible hinge side, for aluminium, steel, wooden and plastic window systems**

1 fanlight tilt fitting, visible hinge side,

Opening width 210/300 mm,  
manual operation by means of hand lever or crank lever.

**Leaf dimensions**

max. leaf weight: AK 210 up to 80 kg / AK 300 up to 120 kg

max. leaf height: 2,200 mm

Leaf width, with 2 hinges: 440 - 1,200 mm (1 stay)  
Leaf width with 4 hinges: 1,201 – 3,600 mm (max. 3 stays)

Space required for rods: AK 210 - approx. 22 mm / AK 300 - 25-29 mm

Opening width: AK 210 - 210 mm / AK 300 - 300 mm

* With an aluminium cover for the rods and corner linkage
* Stay with lock button for taking off its hinges,  
  design for heavy windows with 10 mm rods..
* Additional interlock on both sides for leaf heights over 1,500 mm.

**Tests / standards**

* Corrosion resistance according to **DIN EN 1670, Class 5**
* **RAL** tested

**Finishes**

* Al, E6/C-0 silver anodised
* Al, RAL 9016 powder-coated
* Al powder-coated in special finish

**e.g. WSS fanlight tilt fitting AK 210/300, manual**

**Other elements needed**

* 2 catch and cleaning stays to secure the tilt leaf

**Supplementary information**  
WSS flat shape fanlight opener at [www.wss.de/kataloge.html](http://www.wss.de/kataloge.html)