Turn louvre, manual

**concealed or visible hinge side, for aluminium window systems with sash overlap**

1 manual turn fitting,
with visible or concealed hinge side,
for aluminium window system with a Euro groove and sash overlap.

**Leaf sizes**max. flap weight: 50 kg
max. flap width: 300 mm (ventilation openings > 120 mm)
max. flap height: 2,600 mm

* Installation in floor-to-ceiling ventilation flaps.
* concealed gear for use with standard window handles.
* additional vertical central interlock needed for leaves over 1,301 mm in height

**Finishes**

* Al, E6/C-0 silver anodised
* Al, RAL 9016 powder-coated
* Al powder-coated in special finish

**e.g. WSS turn louvre fitting, manual**

**Other elements needed**

* Tilt window handle
* Rubber stopper for installation on the wall to protect any adjacent dividing wall against the impact of the window handle or on facade posts to protect against damage to the surface.
* DANGER: A concealed opening limiter cannot be installed (available).

**Supplementary information**

see WSS complete catalogue for turn-tilt fittings at [www.wss.de/kataloge.html](http://www.wss.de/kataloge.html)