Parallel opening top-hung fitting for ventilation louvres, manual

**concealed stays, for aluminium window systems**

1 manual parallel opening top-hung fitting for ventilation louvres,  
concealed stays, opening inwards,

for aluminium window systems with a Euro groove and sash overlap.

**Leaf dimensions**

max. leaf weight: 25 kg

max. leaf width: 230 mm

max. leaf height: 2,000 mm

max. opening width: 250 mm

necessary rebate size: 21 x 47 mm

* Operated by a flush-mounted, foldaway lever handle - coating in a matching colour to the louvre.
* Fitted with two vertically arranged, spring-assisted top-hung opening stays on the sides.
* With height adjustment ± 4 mm to allow the fine adjustment of the leaf / gap size on the building site.
* Vertical lock on both sides with ± 1mm compression adjustment
* Horizontal leaf centring ± 3mm.
* Fitting of fully corrosion-resistant materials.

**e.g. WSS parallel opening fitting for ventilation louvres**