Parallel opening top-hung fitting for ventilation louvres, motorised

**concealed stays, for ventilation louvres, for aluminium window system with a Euro groove and sash overlap.**

1 motorised parallel opening top-hung fitting for ventilation louvres,  
concealed stays, opening inwards,

for aluminium window systems with a Euro groove and sash overlap.

**Leaf dimensions**

max. leaf weight: 10 kg

max. leaf width: 150 mm

max. leaf height: 1,700 mm

max. opening width: 250 mm

necessary rebate size: 21 x 47 mm

* Operation by a central concealed louvre motor installed in the louvre.
* Fitted with two vertically arranged, spring-assisted top-hung opening stays on the sides.
* With height adjustment ± 4mm to allow the fine adjustment of the leaf and gap size on the building site.
* Vertical lock on both sides with ± 1mm compression adjustment
* Horizontal leaf centring ± 3mm
* Emergency unlocking mechanism
* Fitting of fully corrosion-resistant materials.

**e.g. WSS parallel opening top-hung fitting for ventilation louvres, motorised**