Parallel opening fitting for ventilation louvres, manual

**concealed stays, for ventilation louvres, for aluminium window systems**

1 manual parallel opening fitting for ventilation louvres, opening inwards, concealed installation, for aluminium window system with a Euro groove and sash overlap.

**Leaf dimensions**

max. leaf weight: 30 kg

max. leaf width: 300 mm

max. leaf height: 2,800 mm

max. opening width: 200 mm

necessary rebate size: 17 x 23 mm

* Operated by a foldaway lever handle mounted flush in the louvre - coating in a matching colour to the louvre.
* Fitted on each side - right and left - with a Tandem PX stay and horizontally at the bottom with a compact control stay.
* With height adjustment +/- 4 mm to allow the fine adjustment of the leaf and gap size on the building site.
* Fitting of fully corrosion-resistant materials.

**e.g. WSS parallel opening fitting for ventilation louvres, manual**