Vertical sliding fitting for double-leaf window

**concealed installation, for double-leaf aluminium window systems, flush-mounted**

1 manual vertical sliding fitting,  
for double-leaf, opposed ventilation leaves, opening inwards,   
concealed installation,

for flush-mounted aluminium window systems.

**Leaf dimensions**

max. leaf weight: 80 kg

min/max. ﻿Leaf width: 875 mm / 2,000 mm

min/max. Leaf height: 800 mm / 1,200 mm

* One-handed operation thanks to handle arranged in the middle of the window leaf.
* The individual window leaves are brought into the tilt position for cleaning purposes
* Horizontal adjustment of the individual window leaves is possible.
* Circumferential lock with ± 1mm compression adjustment
* Fitting of fully corrosion-resistant materials.

**e.g. WSS parallel opening fitting for ventilation louvres, motorised**

**Other elements needed:**

Window handle: see also WSS complete catalogue for turn-tilt fittings at [www.wss.de/kataloge.html](http://www.wss.de/kataloge.html)